**New: I use RX, You use RY**

ssh student@cnalab.cs.adelaide.edu.au

student

minicom --device /lab/routerX -b 9600 -w -8

ENTER

enable

show run (See whether ip address is no or not).

config t

interface Gi 0/0

ip address 192.168.100.X 255.255.255.0

no shutdown

exit

interface Gi 0/1

ip address 192.168.101.X 255.255.255.0

exit

interface Gi 0/0

backup interface Gi 0/1

exit

interface Gi 0/0.1

encap dot1q 10

ip address 192.168.X.1 255.255.255.0

no shutdown

exit

router rip

network 192.168.100.X

network 192.168.101.X

network 192.168.X.1

exit

router ospf 109

network 192.168.100.X 0.0.0.255 area 0

network 192.168.101.X 0.0.0.255 area 0

network 192.168.X.1 0.0.0.255 area 0

exit

exit

ping 192.168.100.Y

show ip route